| Earth Observation Mission CFI Software Visibility Software User Manual |

Public Attributes

# EECFI::MultiStationsExtraInfo Class Reference

Additional information to visibility segments computed for multiple stations. More...

Inheritance diagram for EECFI::MultiStationsExtraInfo:

List of all members.

## Public Attributes
long | numberOfStations
| Number of station from which the satellite is visible during the segment (dummy if extraInfoFlag == false).
vector< long > | stationsInSegment
| Indexes of the stations from which the satellite is visible during the segment (dummy if extraInfoFlag == false).
vector< ANXTime > | multiZdop
| Zero doppler time (dummy if extraInfoFlag == false).

## Detailed Description

Additional information to visibility segments computed for multiple stations.

## Member Data Documentation

vector<ANXTime> EECFI::MultiStationsExtraInfo::multiZdop

Zero doppler time (dummy if extraInfoFlag == false).

long EECFI::MultiStationsExtraInfo::numberOfStations

Number of station from which the satellite is visible during the segment (dummy if extraInfoFlag == false).

vector<long> EECFI::MultiStationsExtraInfo::stationsInSegment

Indexes of the stations from which the satellite is visible during the segment (dummy if extraInfoFlag == false).