| Earth Observation Mission CFI Software DataHandling Software User Manual |

Classes | Enumerations

# EECFI Namespace Reference

## Classes
class | AttFile
| Class for reading/writing attitude generic files. More...
class | AttRec
| Class for storing attitude data. More...
class | AngleModel
| Angle model. More...
class | Asar
| ASAR definition. More...
class | BulbTable
| Class to store the data for one entry read from the IERS bulletin. More...
class | DemPoint
| DEM point class. More...
class | DorisHeader
| Class to store DORIS navigator files header. More...
class | FileModel
| File model. More...
class | HarmonicData
| Harmonic model data. More...
class | HarmonicModel
| Harmonic model. More...
class | MatrixModel
| Matrix model. More...
class | MlstHarmonics
| MLST harmonics. More...
class | MlstNonlinearDrift
| MLST non linear drift. More...
class | ParamModel
| Parameter model. More...
class | SwathGeometry
| Swath geometry data. More...
class | TrackerLimits
| Star tracker limits. More...
class | StfPt
| Swath point coordinates. More...
class | StfVhr
| Class for containing Swath variable header. More...
class | ZonePoint
| Zone point class. More...
class | AttitudeModel
| Attitude model. More...
class | PolarMotionParams
| Polar motion parameters.. More...
class | IersBulletinBrec
| Class to store the data for one entry read from the IERS bulletin B. More...
class | IersBulletinArec
| Class to store the data for one entry read from the IERS bulletin A. More...
class | PolarMotionFormula
| Class to store parameters for polar motion extrapolation formula (from Bulletin A). More...
class | TimeCorrelationFormula
| Class to store parameters for for time correlation extrapolation formula (UT1-UTC) (from Bulletin A). More...
class | IersBulletinBFile
| Class for storing Iers bulletin B file data. More...
class | IersBulletinAFile
| Class for storing Iers bulletin A file data. More...
class | DemConfFile
| Class for reading DEM configuration files. More...
class | DemFile
| Class for reading DEM files. More...
class | DorisFile
| Class for reading/writing DORIS navigator files. More...
class | EEFile
| Abstract basic class for Earth Observation File. More...
class | FileInfo
| Class to select schema from file information. More...
class | IersBulletinFile
| Class for reading Iers bulletins (B -only 2010 format- or A) file data. More...
class | IersFile
| Class for reading Iers bulletin (deprecated, use IersBulletinFile instead). More...
class | OrbitFile
| Class for reading/writing orbit files. More...
class | OsfFile
| Class for reading/writing Orbit Scenario files. More...
class | OsfRec
| Class for containing data structure for Orbit Scenario File records. More...
class | OsvRec
| Class for containing a satellite state vector for a given time. More...
class | PropagPreciseConf
| Class to store the data for numerical propagator configuration. More...
class | SdfFile
| Class for reading Swath defintion files. More...
class | SdfRec
| Class for containing Swath definition data. More...
class | StarFile
| Class for reading star files. More...
class | StarRec
| Class for storing star information. More...
class | StarTracker
| Class for star tracker quaternion. More...
class | StarTrackerConfFile
| Class for reading Star tracker configuration files. More...
class | StarTrackerFile
| Class for reading star tracker files. More...
class | StationFile
| Class for reading Station files. More...
class | StationRec
| Class for storing station information. More...
class | StfFile
| Class for reading/writing Swath Template Files. More...
class | StfRec
| Class to contain a Swath record. More...
class | TleFile
| Class for reading/writing Two Line Elements file. More...
class | TleRec
| Class for containing data structure for Two Line Elements. More...
class | ZoneFile
| Class for reading zone files. More...
class | ZoneRec
| Class for storing zone information. More...
## Enumerations
enum | AttitudeDataTypeEnum { XDCFI_ATT_QUATERNIONS = 0, XDCFI_ATT_ANGLES }
| Attitude data type enumeration. More...
enum | GeomTypeEnum { XDCFI_LINE_GEOM = 0, XDCFI_POINT_GEOM, XDCFI_LIMB_GEOM, XDCFI_DISTANCE_GEOM }
| Geometry types. More...
enum | AsarTypeEnum { XDCFI_NO_ASAR = 0, XDCFI_NARROW_ASAR, XDCFI_WIDE_ASAR }
| ASAR types. More...
enum | TargetRayEnum { XDCFI_NO_REF = 0, XDCFI_STD_REF, XDCFI_USER_REF, XDCFI_PRED_REF, XDCFI_STD_REF_N = 10, XDCFI_USER_REF_N = 20, XDCFI_PRED_REF_N = 30, XDCFI_US76_REF = 300, XDCFI_TROPIC_REF, XDCFI_MID_SUM_REF, XDCFI_MID_WIN_REF, XDCFI_SUBAR_SUM_REF, XDCFI_SUBAR_WIN_REF, XDCFI_LUT_REF = 400, XDCFI_US76_REF_N = 3000, XDCFI_TROPIC_REF_N, XDCFI_MID_SUM_REF_N, XDCFI_MID_WIN_REF_N, XDCFI_SUBAR_SUM_REF_N, XDCFI_SUBAR_WIN_REF_N, XDCFI_LUT_REF_N = 4000 }
| Ray tracing model. More...
enum | SwathTypecEnum { XDCFI_OPEN_SWATH, XDCFI_CLOSED_SWATH }
| Swath types. More...
enum | SwathPointTypeEnum { XDCFI_GEODETIC_SWATH_TYPE, XDCFI_INERTIAL_SWATH_TYPE }
| Swath point types. More...
enum | SwathGeomEnum { XDCFI_SWATH_POINTING_GEOM = 0, XDCFI_SWATH_DISTANCE_GEOM, XDCFI_SWATH_LIMB_GEOM, XDCFI_SWATH_INERTIAL_GEOM, XDCFI_SWATH_SUBSATELLITE_GEOM, XDCFI_SWATH_ASAR_GEOM }
| Swath geometry definition = algoritm. More...
enum | ZoneTypeEnum { XDCFI_NOT_DEFINED = -1, XDCFI_POINT = 0, XDCFI_CIRCLE = 1, XDCFI_SEGMENT = 2, XDCFI_POLYGON = 3 }
| Zone type. More...
enum | AttitudeFrameEnum { XDCFI_SAT_ORBITAL_REF = 0, XDCFI_SAT_NOMINAL_ATT, XDCFI_SAT_ATT, XDCFI_INSTR_ATT }
| Attitude reference frames. More...
enum | CoordinateSystemsEnum { XDCFI_BAR_MEAN_2000 = 1, XDCFI_HEL_MEAN_2000, XDCFI_GEO_MEAN_2000, XDCFI_MEAN_DATE, XDCFI_TRUE_DATE, XDCFI_EARTH_FIXED, XDCFI_BAR_MEAN_1950, XDCFI_GALACTIC, XDCFI_SAT_ACT_REF, XDCFI_QUASI_MEAN_DATE, XDCFI_PSE_TRUE_DATE, XDCFI_PSEUDO_EARTH_FIXED, XDCFI_TOPOCENTRIC, XDCFI_SAT_REF, XDCFI_SAT_REL_REF }
| Coordinate systems. More...
enum | QualityIndexEnum { XDCFI_3_ADJUST_NOMI = 1, XDCFI_4_ADJUST_DMAN, XDCFI_5_INTERP_DGAP, XDCFI_6_EXTRAP_LT1D, XDCFI_7_EXTRAP_1D2D, XDCFI_8_EXTRAP_GT2D, XDCFI_8_EXTRAP_AMAN, XDCFI_Q_INDEX_MAX_ENUM }
| Quality index for Orbit files. More...
enum | SCFDrawModesEnum { XDCFI_SCF_DRAW_SOLID, XDCFI_SCF_DRAW_DASHED, XDCFI_SCF_DRAW_DOTTED, XDCFI_SCF_DRAW_TIMELINE }
| Draw modes for the SCF. More...
enum | SCFFillModesEnum { XDCFI_SCF_FILL_SOLID, XDCFI_SCF_FILL_HOLLOW }
| Fill modes for the SCF. More...
enum | TimeRefDataHandlingEnum { XDCFI_TIME_UNDEF = -1, XDCFI_TIME_TAI, XDCFI_TIME_UTC, XDCFI_TIME_UT1, XDCFI_TIME_GPS }
| Time reference ID. More...
enum | TimeRefOfDataHandlingEnum { XDCFI_TIME_REF_OF_TAI = XDCFI_TIME_TAI, XDCFI_TIME_REF_OF_UTC = XDCFI_TIME_UTC, XDCFI_TIME_REF_OF_UT1 = XDCFI_TIME_UT1, XDCFI_TIME_REF_OF_GPS = XDCFI_TIME_GPS }
| Reference time. More...
enum | ProjectionEnum { XDCFI_READ_DB = 0, XDCFI_GNOMONIC = 1, XDCFI_RECTANGULAR = 2 }
| Type of projections. More...
enum | AttModelEnum { XDCFI_ATT_NONE = 0, XDCFI_ATT_AOCS, XDCFI_ATT_PARAM, XDCFI_ATT_HARMONIC, XDCFI_ATT_FILE, XDCFI_ATT_ANGLE, XDCFI_ATT_MATRIX }
| Attitude model. More...
enum | FileEnum { XDCFI_OSF_FILE, XDCFI_ORBIT_FILE, XDCFI_POF_FILE, XDCFI_ROF_FILE, XDCFI_DORIS_FILE, XDCFI_SDF_FILE, XDCFI_STF_FILE, XDCFI_ATTITUDE_FILE, XDCFI_DEM_CONF_FILE, XDCFI_DEM_FILE, XDCFI_ZONE_FILE, XDCFI_STATION_FILE, XDCFI_STAR_FILE, XDCFI_ATT_STAR_TRACKER_CONF_FILE, XDCFI_ATT_STAR_TRACKER_FILE, XDCFI_IERS_BULLETIN_FILE, XDCFI_TLE_FILE }
| File. More...
enum | FileTypeEnum { XDCFI_UNKNOWN_TYPE = -1, XDCFI_AUTO, XDCFI_ORBIT_CHANGE, XDCFI_STATE_VECTOR, XDCFI_OSF_TYPE, XDCFI_POF_TYPE, XDCFI_ROF_TYPE, XDCFI_DORIS_TYPE, XDCFI_POF_N_DORIS_TYPE, XDCFI_OEF_OSF_TYPE, XDCFI_OEF_POF_TYPE, XDCFI_IERS_B_TYPE, XDCFI_TLE_TYPE, XDCFI_STF_TYPE, XDCFI_DORISPREC_TYPE, XDCFI_DORISPREM_TYPE, XDCFI_ATT_TYPE, XDCFI_SCF_TYPE, XDCFI_PRECISE_PROPAG_TYPE, XDCFI_DEMCFG_TYPE, XDCFI_SATCFG_TYPE, XDCFI_GND_DB_TYPE, XDCFI_SW_DEF_TYPE, XDCFI_ZON_DB_TYPE, XDCFI_STR1ATT_TYPE, XDCFI_IERS_A_TYPE, XDCFI_IERS_B_AND_A_TYPE, XDCFI_FILE_TYPE_MAX_VALUE }
| File type. More...
enum | DemModelEnum { XDCFI_DEM_ACE_MODEL = 0, XDCFI_DEM_GETASSE30_V1, XDCFI_DEM_GETASSE30_V2, XDCFI_DEM_ACE2_9SEC, XDCFI_DEM_NUM_MODELS }
| DEM models. More...
enum | DemGetasseDataSourceEnum { XDCFI_DEM_GETASSE30_SOURCE_ACE, XDCFI_DEM_GETASSE30_SOURCE_MSS, XDCFI_DEM_GETASSE30_SOURCE_EGM96, XDCFI_DEM_GETASSE30_SOURCE_SRTM30 }
| DEM Data Source Types for GETASSE30 V1 and V2. More...
enum | DemAce2DataSourceEnum { XDCFI_DEM_ACE2_SOURCE_SRTM0, XDCFI_DEM_ACE2_SOURCE_SRTM1, XDCFI_DEM_ACE2_SOURCE_SRTM2, XDCFI_DEM_ACE2_SOURCE_SRTM3, XDCFI_DEM_ACE2_SOURCE_SRTM_LAKE, XDCFI_DEM_ACE2_SOURCE_SRTM_GLOBE, XDCFI_DEM_ACE2_SOURCE_SRTM_ALT }
enum | ReadAttErrEnum { XDCFI_CFI_READ_ATT_INIT_PARSER_ERR = 0, XDCFI_CFI_READ_ATT_READ_PARAM_ERR, XDCFI_CFI_READ_ATT_WRONG_FILE_TYPE_ERR, XDCFI_CFI_READ_XML_ATT_NAVIGATION_ERR, XDCFI_CFI_READ_ATT_WRONG_DATA_TYPE_ERR, XDCFI_CFI_READ_ATT_INCONSISTENT_DATA_TYPE_ERR, XDCFI_CFI_READ_ATT_XML_DATA_BLOCK_SIZE_ERR, XDCFI_CFI_READ_ATT_WRONG_REF_FRAME_ERR, XDCFI_CFI_READ_ATT_READ_LIST_ERR, XDCFI_CFI_READ_ATT_TIME_CONV_ERR, XDCFI_CFI_READ_ATT_MEMORY_ERR, XDCFI_CFI_READ_ATT_CLEANUP_PARSER_ERR, XDCFI_CFI_READ_ATT_WRONG_TIME_REF_ERR, XDCFI_CFI_READ_ATT_WRONG_QUATERNION_ERR, XDCFI_CFI_READ_ATT_WRONG_ANGLE_ERR, XDCFI_CFI_READ_ATT_MAX_GAP_ERR }
| Error codes list of AttFile.read. More...
enum | PrecisePropagUserFlagEnum { XDCFI_DEFAULT_VALUES = 0, XDCFI_USER_VALUES = 1 }
| User flag for precise propagator. More...
enum | PrecisePropagSelectionFlagEnum { XDCFI_NOT_SELECT = 0, XDCFI_SELECT = 1 }
| Flag to select or not contributions to precise propagator. More...
enum | PrecisePropagSgaFlagEnum { XDCFI_SGA_USE_PARAMETERS = 0, XDCFI_SGA_READ_VALUES_FROM_FILE = 1 }
| Flag to select if SGA values are taken for input parameters or read from file. More...
enum | XDSatIdEnum { XDCFI_SAT_DEFAULT = 0, XDCFI_SAT_DEFAULT1 = 1, XDCFI_SAT_DEFAULT2 = 2, XDCFI_SAT_DEFAULT3 = 3, XDCFI_SAT_DEFAULT4 = 4, XDCFI_SAT_DEFAULT5 = 5, XDCFI_SAT_DEFAULT6 = 6, XDCFI_SAT_DEFAULT7 = 7, XDCFI_SAT_DEFAULT8 = 8, XDCFI_SAT_DEFAULT9 = 9, XDCFI_SAT_ERS1 = 11, XDCFI_SAT_ERS2 = 12, XDCFI_SAT_ENVISAT = 21, XDCFI_SAT_METOP1 = 31, XDCFI_SAT_METOP2 = 32, XDCFI_SAT_METOP3 = 33, XDCFI_SAT_CRYOSAT = 41, XDCFI_SAT_ADM = 51, XDCFI_SAT_GOCE = 61, XDCFI_SAT_SMOS = 71, XDCFI_SAT_TERRASAR = 81, XDCFI_SAT_EARTHCARE = 91, XDCFI_SAT_SWARM_A = 101, XDCFI_SAT_SWARM_B = 102, XDCFI_SAT_SWARM_C = 103, XDCFI_SAT_SENTINEL_1A = 110, XDCFI_SAT_SENTINEL_1B = 111, XDCFI_SAT_SENTINEL_2 = 112, XDCFI_SAT_SENTINEL_3 = 113, XDCFI_SAT_SEOSAT = 120, XDCFI_SAT_SENTINEL_1C = 125, XDCFI_SAT_SENTINEL_2A = 126, XDCFI_SAT_SENTINEL_2B = 127, XDCFI_SAT_SENTINEL_2C = 128, XDCFI_SAT_SENTINEL_3A = 129, XDCFI_SAT_SENTINEL_3B = 130, XDCFI_SAT_SENTINEL_3C = 131, XDCFI_SAT_GENERIC = 200, XDCFI_SAT_GENERIC_GEO = 300, XDCFI_SAT_MTG = 301 }
| Satellite ID. More...
enum | XDBulletinTypeEnum { XDCFI_BULLETIN_A = 0, XDCFI_BULLETIN_B }
| Bulletin type: A or B. More...
enum | DemCacheTypeEnum { XDCFI_NO_CACHE = 0, XDCFI_PRELOAD_CACHE, XDCFI_FIFO_CACHE }
| DEM cache type. More...

## Enumeration Type Documentation

enum EECFI::AsarTypeEnum

ASAR types.

Enumerator:

  XDCFI_NO_ASAR |
  XDCFI_NARROW_ASAR |
  XDCFI_WIDE_ASAR |

enum EECFI::AttitudeDataTypeEnum

Attitude data type enumeration.

Enumerator:

  XDCFI_ATT_QUATERNIONS |
  XDCFI_ATT_ANGLES |

enum EECFI::AttitudeFrameEnum

Attitude reference frames.

Enumerator:

  XDCFI_SAT_ORBITAL_REF |
  XDCFI_SAT_NOMINAL_ATT |
  XDCFI_SAT_ATT |
  XDCFI_INSTR_ATT |

enum EECFI::AttModelEnum

Attitude model.

Enumerator:

  XDCFI_ATT_NONE |
  XDCFI_ATT_AOCS |
  XDCFI_ATT_PARAM |
  XDCFI_ATT_HARMONIC |
  XDCFI_ATT_FILE |
  XDCFI_ATT_ANGLE |
  XDCFI_ATT_MATRIX |

enum EECFI::CoordinateSystemsEnum

Coordinate systems.

Enumerator:

  XDCFI_BAR_MEAN_2000 | Barycentric Mean of 2000.0 coordinate system.
  XDCFI_HEL_MEAN_2000 | Heliocentric Mean of 2000.0 coordinate system.
  XDCFI_GEO_MEAN_2000 | Geocentric Mean of 2000.0 coordinate system.
  XDCFI_MEAN_DATE | Mean of date coordinate system.
  XDCFI_TRUE_DATE | True of date coordinate system.
  XDCFI_EARTH_FIXED | Earth Fixed coordinate system.
  XDCFI_BAR_MEAN_1950 | Barycentric Mean of 2000.0 coordinate system.
  XDCFI_GALACTIC | Galactic coordinate system.
  XDCFI_SAT_ACT_REF | Satellite relative actual reference cs.
  XDCFI_QUASI_MEAN_DATE | Quasi-Mean of Date coordinate system.
  XDCFI_PSE_TRUE_DATE | Pseudo-True of Date coordinate system.
  XDCFI_PSEUDO_EARTH_FIXED | Quasi-True of Date coordinate system.
  XDCFI_TOPOCENTRIC | Topocentric coordinate system.
  XDCFI_SAT_REF | Satellite reference coordinate system.
  XDCFI_SAT_REL_REF | Satellite relative reference coordinate system.

enum EECFI::DemAce2DataSourceEnum

Enumerator:

  XDCFI_DEM_ACE2_SOURCE_SRTM0 |
  XDCFI_DEM_ACE2_SOURCE_SRTM1 |
  XDCFI_DEM_ACE2_SOURCE_SRTM2 |
  XDCFI_DEM_ACE2_SOURCE_SRTM3 |
  XDCFI_DEM_ACE2_SOURCE_SRTM_LAKE |
  XDCFI_DEM_ACE2_SOURCE_SRTM_GLOBE |
  XDCFI_DEM_ACE2_SOURCE_SRTM_ALT |

enum EECFI::DemCacheTypeEnum

DEM cache type.

Enumerator:

  XDCFI_NO_CACHE |
  XDCFI_PRELOAD_CACHE |
  XDCFI_FIFO_CACHE |

enum EECFI::DemGetasseDataSourceEnum

DEM Data Source Types for GETASSE30 V1 and V2.

Enumerator:

  XDCFI_DEM_GETASSE30_SOURCE_ACE |
  XDCFI_DEM_GETASSE30_SOURCE_MSS |
  XDCFI_DEM_GETASSE30_SOURCE_EGM96 |
  XDCFI_DEM_GETASSE30_SOURCE_SRTM30 |

enum EECFI::DemModelEnum

DEM models.

Enumerator:

  XDCFI_DEM_ACE_MODEL |
  XDCFI_DEM_GETASSE30_V1 |
  XDCFI_DEM_GETASSE30_V2 |
  XDCFI_DEM_ACE2_9SEC |
  XDCFI_DEM_NUM_MODELS |

enum EECFI::FileEnum

File.

Enumerator:

  XDCFI_OSF_FILE |
  XDCFI_ORBIT_FILE |
  XDCFI_POF_FILE |
  XDCFI_ROF_FILE |
  XDCFI_DORIS_FILE |
  XDCFI_SDF_FILE |
  XDCFI_STF_FILE |
  XDCFI_ATTITUDE_FILE |
  XDCFI_DEM_CONF_FILE |
  XDCFI_DEM_FILE |
  XDCFI_ZONE_FILE |
  XDCFI_STATION_FILE |
  XDCFI_STAR_FILE |
  XDCFI_ATT_STAR_TRACKER_CONF_FILE |
  XDCFI_ATT_STAR_TRACKER_FILE |
  XDCFI_IERS_BULLETIN_FILE |
  XDCFI_TLE_FILE |

enum EECFI::FileTypeEnum

File type.

Enumerator:

  XDCFI_UNKNOWN_TYPE |
  XDCFI_AUTO |
  XDCFI_ORBIT_CHANGE |
  XDCFI_STATE_VECTOR |
  XDCFI_OSF_TYPE |
  XDCFI_POF_TYPE |
  XDCFI_ROF_TYPE |
  XDCFI_DORIS_TYPE |
  XDCFI_POF_N_DORIS_TYPE |
  XDCFI_OEF_OSF_TYPE |
  XDCFI_OEF_POF_TYPE |
  XDCFI_IERS_B_TYPE |
  XDCFI_TLE_TYPE |
  XDCFI_STF_TYPE |
  XDCFI_DORISPREC_TYPE |
  XDCFI_DORISPREM_TYPE |
  XDCFI_ATT_TYPE |
  XDCFI_SCF_TYPE |
  XDCFI_PRECISE_PROPAG_TYPE |
  XDCFI_DEMCFG_TYPE |
  XDCFI_SATCFG_TYPE |
  XDCFI_GND_DB_TYPE |
  XDCFI_SW_DEF_TYPE |
  XDCFI_ZON_DB_TYPE |
  XDCFI_STR1ATT_TYPE |
  XDCFI_IERS_A_TYPE |
  XDCFI_IERS_B_AND_A_TYPE |
  XDCFI_FILE_TYPE_MAX_VALUE |

enum EECFI::GeomTypeEnum

Geometry types.

Enumerator:

  XDCFI_LINE_GEOM |
  XDCFI_POINT_GEOM |
  XDCFI_LIMB_GEOM |
  XDCFI_DISTANCE_GEOM |

enum EECFI::PrecisePropagSelectionFlagEnum

Flag to select or not contributions to precise propagator.

Enumerator:

  XDCFI_NOT_SELECT | Do not select contribution.
  XDCFI_SELECT | Select contribution.

enum EECFI::PrecisePropagSgaFlagEnum

Flag to select if SGA values are taken for input parameters or read from file.

Enumerator:

  XDCFI_SGA_USE_PARAMETERS | Use input parameters.
  XDCFI_SGA_READ_VALUES_FROM_FILE | Read values from files.

enum EECFI::PrecisePropagUserFlagEnum

User flag for precise propagator.

Enumerator:

  XDCFI_DEFAULT_VALUES | Use predefined default values for some parameters.
  XDCFI_USER_VALUES | Use values introduced by user.

enum EECFI::ProjectionEnum

Type of projections.

Enumerator:

  XDCFI_READ_DB | Read projection from DB file.
  XDCFI_GNOMONIC | Use gnomonic projection.
  XDCFI_RECTANGULAR | Use rectangular projection.

enum EECFI::QualityIndexEnum

Quality index for Orbit files.

Enumerator:

  XDCFI_3_ADJUST_NOMI | Adjusted out of orbit manoeuvre period.
  XDCFI_4_ADJUST_DMAN | Adjusted during an orbit manoeuvre.
  XDCFI_5_INTERP_DGAP | Interpolated during a data gap.
  XDCFI_6_EXTRAP_LT1D | Extrapolated from less than 1 day.
  XDCFI_7_EXTRAP_1D2D | Extrapolated from more than 1 day, but less than 2 days.
  XDCFI_8_EXTRAP_GT2D | Extrapolated from more than 2 days.
  XDCFI_8_EXTRAP_AMAN | Extrapolated after an orbit manoeuvre.
  XDCFI_Q_INDEX_MAX_ENUM | Number of defined values (+1).

enum EECFI::ReadAttErrEnum

Error codes list of AttFile.read.

Enumerator:

  XDCFI_CFI_READ_ATT_INIT_PARSER_ERR |
  XDCFI_CFI_READ_ATT_READ_PARAM_ERR |
  XDCFI_CFI_READ_ATT_WRONG_FILE_TYPE_ERR |
  XDCFI_CFI_READ_XML_ATT_NAVIGATION_ERR |
  XDCFI_CFI_READ_ATT_WRONG_DATA_TYPE_ERR |
  XDCFI_CFI_READ_ATT_INCONSISTENT_DATA_TYPE_ERR |
  XDCFI_CFI_READ_ATT_XML_DATA_BLOCK_SIZE_ERR |
  XDCFI_CFI_READ_ATT_WRONG_REF_FRAME_ERR |
  XDCFI_CFI_READ_ATT_READ_LIST_ERR |
  XDCFI_CFI_READ_ATT_TIME_CONV_ERR |
  XDCFI_CFI_READ_ATT_MEMORY_ERR |
  XDCFI_CFI_READ_ATT_CLEANUP_PARSER_ERR |
  XDCFI_CFI_READ_ATT_WRONG_TIME_REF_ERR |
  XDCFI_CFI_READ_ATT_WRONG_QUATERNION_ERR |
  XDCFI_CFI_READ_ATT_WRONG_ANGLE_ERR |
  XDCFI_CFI_READ_ATT_MAX_GAP_ERR |

enum EECFI::SCFDrawModesEnum

Draw modes for the SCF.

Enumerator:

  XDCFI_SCF_DRAW_SOLID |
  XDCFI_SCF_DRAW_DASHED |
  XDCFI_SCF_DRAW_DOTTED |
  XDCFI_SCF_DRAW_TIMELINE |

enum EECFI::SCFFillModesEnum

Fill modes for the SCF.

Enumerator:

  XDCFI_SCF_FILL_SOLID |
  XDCFI_SCF_FILL_HOLLOW |

enum EECFI::SwathGeomEnum

Swath geometry definition = algoritm.

Enumerator:

  XDCFI_SWATH_POINTING_GEOM |
  XDCFI_SWATH_DISTANCE_GEOM |
  XDCFI_SWATH_LIMB_GEOM |
  XDCFI_SWATH_INERTIAL_GEOM |
  XDCFI_SWATH_SUBSATELLITE_GEOM |
  XDCFI_SWATH_ASAR_GEOM |

enum EECFI::SwathPointTypeEnum

Swath point types.

Enumerator:

  XDCFI_GEODETIC_SWATH_TYPE |
  XDCFI_INERTIAL_SWATH_TYPE |

enum EECFI::SwathTypecEnum

Swath types.

Enumerator:

  XDCFI_OPEN_SWATH |
  XDCFI_CLOSED_SWATH |

enum EECFI::TargetRayEnum

Ray tracing model.

Enumerator:

  XDCFI_NO_REF |
  XDCFI_STD_REF |
  XDCFI_USER_REF |
  XDCFI_PRED_REF |
  XDCFI_STD_REF_N |
  XDCFI_USER_REF_N |
  XDCFI_PRED_REF_N |
  XDCFI_US76_REF |
  XDCFI_TROPIC_REF |
  XDCFI_MID_SUM_REF |
  XDCFI_MID_WIN_REF |
  XDCFI_SUBAR_SUM_REF |
  XDCFI_SUBAR_WIN_REF |
  XDCFI_LUT_REF |
  XDCFI_US76_REF_N |
  XDCFI_TROPIC_REF_N |
  XDCFI_MID_SUM_REF_N |
  XDCFI_MID_WIN_REF_N |
  XDCFI_SUBAR_SUM_REF_N |
  XDCFI_SUBAR_WIN_REF_N |
  XDCFI_LUT_REF_N |

enum EECFI::TimeRefDataHandlingEnum

Time reference ID.

Enumerator:

  XDCFI_TIME_UNDEF |
  XDCFI_TIME_TAI |
  XDCFI_TIME_UTC |
  XDCFI_TIME_UT1 |
  XDCFI_TIME_GPS |

enum EECFI::TimeRefOfDataHandlingEnum

Reference time.

Enumerator:

  XDCFI_TIME_REF_OF_TAI |
  XDCFI_TIME_REF_OF_UTC |
  XDCFI_TIME_REF_OF_UT1 |
  XDCFI_TIME_REF_OF_GPS |

enum EECFI::XDBulletinTypeEnum

Bulletin type: A or B.

Enumerator:

  XDCFI_BULLETIN_A |
  XDCFI_BULLETIN_B |

enum EECFI::XDSatIdEnum

Satellite ID.

Enumerator:

  XDCFI_SAT_DEFAULT |
  XDCFI_SAT_DEFAULT1 |
  XDCFI_SAT_DEFAULT2 |
  XDCFI_SAT_DEFAULT3 |
  XDCFI_SAT_DEFAULT4 |
  XDCFI_SAT_DEFAULT5 |
  XDCFI_SAT_DEFAULT6 |
  XDCFI_SAT_DEFAULT7 |
  XDCFI_SAT_DEFAULT8 |
  XDCFI_SAT_DEFAULT9 |
  XDCFI_SAT_ERS1 |
  XDCFI_SAT_ERS2 |
  XDCFI_SAT_ENVISAT |
  XDCFI_SAT_METOP1 |
  XDCFI_SAT_METOP2 |
  XDCFI_SAT_METOP3 |
  XDCFI_SAT_CRYOSAT |
  XDCFI_SAT_ADM |
  XDCFI_SAT_GOCE |
  XDCFI_SAT_SMOS |
  XDCFI_SAT_TERRASAR |
  XDCFI_SAT_EARTHCARE |
  XDCFI_SAT_SWARM_A |
  XDCFI_SAT_SWARM_B |
  XDCFI_SAT_SWARM_C |
  XDCFI_SAT_SENTINEL_1A |
  XDCFI_SAT_SENTINEL_1B |
  XDCFI_SAT_SENTINEL_2 |
  XDCFI_SAT_SENTINEL_3 |
  XDCFI_SAT_SEOSAT |
  XDCFI_SAT_SENTINEL_1C |
  XDCFI_SAT_SENTINEL_2A |
  XDCFI_SAT_SENTINEL_2B |
  XDCFI_SAT_SENTINEL_2C |
  XDCFI_SAT_SENTINEL_3A |
  XDCFI_SAT_SENTINEL_3B |
  XDCFI_SAT_SENTINEL_3C |
  XDCFI_SAT_GENERIC |
  XDCFI_SAT_GENERIC_GEO |
  XDCFI_SAT_MTG |

enum EECFI::ZoneTypeEnum

Zone type.

Enumerator:

  XDCFI_NOT_DEFINED | The zone is not defined as an input and must be read from a file.
  XDCFI_POINT | The zone is a point (resulting segments will be of zero duration).
  XDCFI_CIRCLE | The zone is a circle defined by its centre point and its radius.
  XDCFI_SEGMENT | The zone is a segment defined by its two extremes.
  XDCFI_POLYGON | The zone is a polygon.